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The Penn Conventional Reel Project - Help Fill in the Blanks 



What we're trying to build here is a complete data
 listing for Penn conventional reels.
Ultimately this will include a cross reference showing what parts are interchangeable 
with which reels, including Newell, Accurate, Tiburon and other aftermarket parts suppliers.

If you can add anything to the information below please post it.
--------------------------------------------------------------------------------
Reel number followed by no letter = Plastic Spool
Reel number followed by "M" = Chromed Steel Spool
Reel number followed by "L" = Aluminum Spool
Reel number followed by "LH" = Left Hand

Penn Standard Conventional's

Penn 15 - ???
Direct drive
, no drag

25 Monofil
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Gear
 Ratio: 3:1 Line
:Capacity: 15 lb 400 yds Weight:13.5 oz
First Year Manf.: Late 1950's Discontinued by Penn: Early 70's

26 Monofil
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Gear Ratio: 3:1 Line:Capacity: 15 lb 450 yds Weight:15 oz
First Year Manf.: Late 1950's Discontinued by Penn: Early 70's

27 Monofil
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Gear Ratio: 3:1 Line:Capacity: 15 lb 300 yds Weight:12.5 oz
First Year Manf.: Late 1950's Discontinued by Penn: Early 70's

49 Mariner
Gear Ratio: 3.5:1, 300 yds of 30# mono, Weight 30 oz
add "L" for aluminum spool (a left handed version was made sometime around 1941 which was also designatel by a "L")


Longbeach Series:
60 Longbeach, Smallest of the longbeach series, 500 yds. of 15lb., 2.5 to 1 ratio
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65 Longbeach
67 Super Longbeach - 300 yards of 40# test mono
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66 Super Longbeach
68 SuperLongbeach - 500yds of 40 lb., 2.5 : 1 ratio ----(trolling reel)
[image: image16.jpg]




77 Sea-Hawk - inexpensive bakalite reel
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78 Sea-Scamp - inexpensive bakalite reel

79 Sea-Mate

Penn 80
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Gear Ratio: 3:1 Line: linen Capacity: 15 lb 
300 yds Weight: 12.5 oz


85 Sea Boy - inexpensive reel
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Gear Ratio: 3:1 Line Capacity: 20 lbs 400 yds Weight: 15 oz 
First Year Manufactured: Before 1941 Discontinued by Penn: Late 1980's
Seaboy Series - A fishermen's favorite for salt
 water
 and inland river 
fishing. All external parts of that reel were made of solid brass and 
corrosion resistant, with a plastic spool. Sliding click.

99 Silver Beach - 3 to 1 ratio
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Surfmaster Series - Bushing
100 Narrow Spool
150 Mid size spool
*Note - the Accurate AF-145 145 Midsize Squidder/Surfmaster after market frame does not fit with the standard Penn 150 spool. No spool was manufactured by accurate for the 150 Surfmaster
200 Standard Surfmaster
Add "L" for aluminum spool
Surfmaster series has bushings.

250

130 Sailfisher

Squidder Series
140 Standard Squidder, Line Capacity: 350 yds/20Lb.. Gear Ratio: 3:1.
145 Mid size spool
*Note - the Accurate AF-145 145 Midsize Squidder/Surfmaster after market frame does not fit with the standard Penn 145 spool, you must have the matching, and hard to find, Accurate spool.
146 Narrow Spool
Add "LH" for left hand retrieve
Squidder series has bearings.

149, Super Mariner
Add "L" for aluminum spool

Beachmaster Series
155
156 - A 155 without the star drag was manufactured for a short time.
160 - ratio 2.8:1, 150 Yards 30 Lb Dacron
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165 Beachmaster
Add "L" for aluminum spool
Beachmaster series has bushings

180 Baymaster (SPOOL IS 1 9/16" WIDE),
250 yds. of 18 lb, 2.8 to 1 ratio
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185 Baymaster (up to 1970),
185 Seaboy (1990+),

190 Seaboy

249 Mariner

349 Master Mariner
349H Master Mariner
349HC Master Mariner

259 Live Bait Caster
267 Long Beach
268 Long Beach

285 Delmar - bacalite sides
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Jigmaster Series:
500 Jigmaster 4-1 gear ratio, 275 yards of 30 lb
500S Jigmaster - This version has some parts that do not fit the standard 500, the bushings for example
bars and base are the same, unsure about the red aluminum spool
501 Jigmaster Narrow Spool
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505HS Jigmaster High Speed - 5-1 gear ratio, 275 yards of 30 lb
506HS Jigmaster High Speed Narrow Spool
Add "L" for aluminum spool
Add "LH" for left hand retrieve

970 Mag Power
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980 Mag Power
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990 Mag Power
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Penn Level Lines

9 Peerless
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9M Monofil
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9MS Peerless Monofil 400 of 12#

10 Mag Tuned, 4 to 1 ratio, 275 of 15# mono.
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Gear Ratio: 4:1Line: 15 lbCapacity:275 ydsWeight: 14 oz. First Year Manufactured.: Early 1980's Discontinued by Penn: 2002

109 Peer levelwind, Capacity 275 - 15LB mono, Ratio 3.75 / 1
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109LH - left hand retrieve
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109M, Peer, Monofil

209 Peer, Peer, Monofil Sr. Level Wind reel. Gear ratio 3-1 line cap. 320yds.of 20
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209M
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209MF - 250 of 36# Nylon - 300 mono
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210M Mag Tuned
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210 MS, Levelwind, Ball Bearings, Gear Ratio 4:1, 350 YDS./20LB

309 Levelwind, Gear Ratio 3.0/1 . Capacity 30 LB ? 350 to 375 YDS
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309M Super Peer

310GTi Super Levelwind Graphite

320GTi Super Levelwind Graphite
320GT2 Super Levelwind Graphite Next Gen.
320LD Super Levelwind Graphite Leverdrag

321GTi-LH Super Levelwind Graphite
330GTi Super Levelwind Graphite
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330LD Super Levelwind Graphite Leverdrag

340GTi Super Levelwind Graphite 4/0

345GTi Super Levelwind Graphite 5/0

350M Leveline
Reel uses a rotating bar with a twist in it rather that a standard levelwind
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The 350 has bushings.
Same spool as the 200 Surfmaster and 155 Beachmaster
Takes the same base as the 200, 155 and the 140 Squidder
I've never been able to find a solid replacement bar for the two posts in the rear - if someone knows of one, please post it.
*Replace the chromed steel spool with the Penn or Newell aluminium spool, the bushings with the Newell teflon bushings, the rear posts with a Newell bar and the stamped steel base with a Newell base (Newell parts are the same as for the 140 Squidder and 200 Surfmaster), mag the reel and it becomes a very capable beach
 casting reel.

Baitcasters

See International Section for Int. Baitcasters
920 Levelmatic Narrow Spool w/CB-handle 20LB = 120 YDS, 4 to 1 ratio
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930 Levelmatic w/CB-handle

940 Levelmatic w/P-handle

1000 Baitcaster

2000 Baitcaster

Senators
110 1/0 Senator Light Tackle
 Trolling

111 2/0 Senator Light Tackle Trolling

112 (3/0) Senator Light Tackle Trolling
112H (3/0) Special
 Senator Light Tackle Trolling

113 (4/0) Senator Light Tackle Trolling
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113H (4/0) Special Senator Light Tackle Trolling
113HN (4/0) Senator Baja Special
113HL (4/0) Special Senator Light Tackle Trolling
113HLW (4/0) Special Senator Light Tackle Trolling
113HSP (4/0) Special Senator Wire Lining

114 (6/0) Senator Light Tackle Trolling
114H (6/0) Special Senator Light Tackle Trolling
114HL (6/0) Special Senator Light Tackle Trolling
114HLW (6/0) Special Senator Light Tackle Trolling

115L (9/0) Senator Medium Tackle Trolling

116A (10/0) Senator Heavy Tackle Trolling
116L (12/0) Senator Heavy Tackle Trolling

117L (14/0) Senator Ex. Heavy Tackle Trolling

118 (16/0) Senator Ex. Heavy Tackle Trolling

Offshore Leverdrag Models
GLD 20
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GLD 20ii

GLD 30
GLD 30ii
GLD 50ii

10KG Formula Graphite Leverdrag 2-Speed
10LD Formula Graphite Leverdrag

15KG Formula Graphite Leverdrag 2-Speed
15LD Formula Graphite Leverdrag

225LD Graphite Leverdrag
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24KG Formula Graphite Leverdrag 2-Speed
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245LD Graphite Leverdrag

246LD Graphite Leverdrag

Misc Offshore/Trolling
25GLS GLS series Graphite
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40GLS GLS series Graphite

45GLS GLS series Graphite

49L Super Mariner

525GS Graphite Series
525MAG Graphite Series
[image: image53.jpg]




525MAG-T Graphite Series

535GS Graphite Series
535MAG Graphite Series

545GS Graphite Series
545MAG Graphite Series

555GS Graphite Series
555MAG Graphite Series

855LC Linecounter
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875LC Linecounter

895LC Linecounter

PENN COMMANDER 30LW ratio 4.2 : 1, 330 yards 30lb
[image: image55.jpg]




No data for the following reels:
#6 International
14 Atlantic
125 Seagate

Matching size drag washers 

10.60,65,85,99,100,110,140,145,146,149,150,200,285,910,920,930,940, 860,870, and 880
9,109, 149,155,25,160,180,26,27,209, AND 350
210, 309, 500SL,501, 505, 506, 500, AND 112H
113H,113HSP,113HL,113HLW,340GTI,AND 345GTI

Matching Spools
100,180,185,190 and possibly more
79,80,85,285 and possibly more
60,111-285 and possibly more
49-149 and possibly more
Spool part # 29L-150 - fits 150, 160, 165 maybe more.

Matching side rings
155,160 and 180 and possibly more
66,67 and 68 and possibly more
2/0 111 Senator, 60 Longbeach, 85 & 285

Matching Bushings
Surfmaster series, Beachmaster series, 350 Leveline, maybe more 

Matching Base Plate
Penn 30-66 reel stand will fit the Penn reels 66,112H,150, 209 and 309

Newell graphite RB2/15 (Plastic)stand kit with clamp & Stainless Steel clamp mounting screws fits the Penn 112H 3/0 High Speed Senator, 145 midsized Squidder, 150 Surfmaster , 160 Beachmaster, Albacore Special ( a converted Penn Jigmaster with a S99 spool this stand & Newell SP1 posts) or any Penn reel using the 29-65 or 29-66 stand & fits the Newell 229 Or 332 with the short screwed frame ,a set of 4 Newell short frame screws. The Penn stand screws will be too short

Newell Graphite ( Plastic) SP4 Suport spacer bars. Parts have " Newell on them in bold white letters , note change in style
 of the letters they are slanted now. One post has a metal strip so the line will not cut into it. These fit the 220 or 322 Newell reels using short screws or the following Penn reels 501,506,349,149,49, & the 110 1/0 Senator using longer screws.

<Thanks to Zim for all the following Accurate and Tiburon data>

Accurate parts cross reference:

AccuFrames

AF-112 3/O Senator Frame 
AF-113 4/O Senator Frame 
AF-113n 4/O Narrow Senator Frame 
AF-113nk 113 Narrow Kit, Frame & Spool 
AF-113sp Narrow 4/O Spool 
AF-113w 4/O Wide Senator Frame 
AF-114 6/O Senator Frame 
AF-114w 6/O Senator Wide Frame 
AF-115 9/O Senator Frame 
AF-12i International 12 Frame 
AF-12wi International 12 Wide Frame 
AF-140 140 AccuFrame 
AF-145 145 Midsize Squidder - does not fit with the standard Penn spool, you must have the matching, and hard to find, Accurate spool.
AF-146 Squidder 146 Jr. AccuFrame 
AF-30i International 30 Frame 
AF-500 Jigmaster 500 Frame 
AF-501 Jigmaster 501 AccuFrame 
AF-50i International 50 Frame 
AF-50wi International 50 Wide Frame 
AF-6i International 6 Frame 
AF-99 Jigmaster 99 Mid-size Frame 
AF-99k Jigmaster 99 Mid-size Kit, Frame & Spool 
AF-99kh Jigmaster 99 Mid-size High Speed 505 Kit, Frame & Spool 
AF-99sp Jigmaster 99 spool for 500 & 501 
AF-99sph Jigmaster 99 High Speed spool for 505 & 506 

AccuPlates
ASP-140 AccuPlates for Penn Squidder 140 & 146. 
ASP-40 AccuPlates for Penn Senator 113H, 113HLW. 
ASP-500 AccuPlates for Penn Jigmaster 500 & 501. 
ASP-505 AccuPlates for Penn Jigmaster 505 & 506. 
ASP-6o AccuPlates for Penn Senator 114H, 114HLW. 

Handles
H-4o 4/O Power Handle fits: 4/Os, 349. 
H-500 Jigmaster 500 Power Handle fits: Squidder, Jigmaster, 3/O's, International 12T, Boss 197, Boss 270, Boss 870 
H-6o 6/O Power Handle fits: 6/O's, 9/O's. 
HC-500 Jigmaster 500 Power Handle fits: Squidder, Jigmaster, 3/O's, International 12T, Boss 197, Boss 270, Boss 870 

Aftermarket Clamps

C-30 C-30 Clamp fits this reel: 30T 
C-40 C-40 Clamp fits these reels: 6, 12H, 12W, 66, 67, 68, 99, 111, 112, 112H ,113, 113H, 113HL, 113HLW, 140, 145, 150, 200, 209, 210, 285, 320GTI, 330GTI, 12T, 30, 309, 350, 500, 500L, 500S, 505HS, 506HS, 970, 25GLS, & 40GLS 
C-51 C-51 Clamp fits these reels: 20, 20T, 49, 49L, 100, 110, 146, 146L, 349, 349H, 349HC, 501, & 501L 
C-60 C-60 Clamp fits these reels: 114, 114H, 114HL, 115, 115L, 114HLW, 30TW, 30SW, 50, 50T, 50S, 50W, 50TW, & 50SW 
C-60l C-60 Clamp w/lanyard fits these reels: 114, 114H, 114HL, 115, 115L, 114HLW, 30TW, 30SW, 50, 50T, 50S, 50W, 50TW, & 50SW 
C-80 C-80 Clamp w/lanyard fits these reels: 80, 80T, 80S, 80W, 80TW, 80SW, 80STW, 130, 130H, 130S, & 130ST 

Gears

G-40 Senator 113H - High Speed 4 to 1 Gears 
G-60 Senator 114H - High Speed 3.25 to 1 Gears 

Miscellaneous Accurate Parts

AF-405 140, 500, 3/0 & 4/0 clicker parts 
AF-40pk 3/0, 4/0, 6/0 & 90 AccuFrame screws and clamp 
AF-500pk 140, 146, 500, 99 & 501 AccuFrame screws and clamp 
AF-605 6/0 & 9/0 clicker parts 
ASP-40h 4/O sideplate bearings and screws 
ASP-55h 140 & 505 sideplate bearings and screws 
ASP-5h 500 & 3/0 sideplate bearings and screws 
ASP-60h 6/O sideplate bearings and screws

TIBURON parts cross reference

TIBURON
TC965 Clamp Kit
Fits Penn 965 
Black

T-Bar Lite Articulated Reel Handles
MODEL
FITS REEL MODELS

TB16
PENN International 16S

TB300
PENN International 6, 12H, 12T, Senator 112, Jigmasters & Squidders

TB300
PRO GEAR 200 Series & 2000 Pacifica Series

TB 400
PENN Senator 113 & GLS
TB1015
PENN 10KG & 15KG
TB1250
PENN International 20T, 30T, 30TW, 30SW, 50T, 50S, 50TW & 50SW 
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Quote:

Originally Posted by sealegs 

has anyone done something similar for spinning reels?

sealegs. 
Scott at Scotts Bait and tackle has a Penn reels site 
and he has an extensive library of penn parts both 
spinning and conventional. The older Penn 700 series 
parts are compatable with the newer Z series.
List of all Penn Reels
Loads slowly 
ScottsBt Penn Reel Parts List

Penns Web site Parts lists


Charkbait has Accurate Newell and Baker parts but cautions that 
accurate will probably cease production of these aftermarket
penn products in the near future if they havent already
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Beth and Carl Newell at his workshop



Edit 
Rest in Peace Carl
http://www.stripers247.com/phpBB2/showthread.php?t=15638 
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the > 6500>7500>8500 & the 9500ss was discontinued and the new replacement is the 650ss thru 950ss which is now available. 950= ($150.00). same gear ratio as it's predecessor however the fail free bail spring may be an added treat as the older models were suceptable to failure. curious if the handle is still metal or a composite like some of the lesser models like the cs105's.

9500

Gear Ratio: 4.2:1
Line Capacity: 300/30
Weight: 32 oz 
Techno-Balanced Rotor 
Full Metal Body Construction 
Infinite Anti-Reverse Roller Bearing 
Leveline Spool Wrap System 
5 Stainless Steel Ball Bearings 
Sealed Drag Knob 
Fail Free Bail Spring 
Stainless Steel Main Shaft 
Corrosion-Resistant, Gold-Anodized, Machined Handle

this is the ssm series as the ssg series goes from 420 - 430 - 440 - 450 -550ssg as these are the smaller of the spinfisher series. 
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Re: The Penn Reel Project - Help Fill in the Blanks 



Quote:

Originally Posted by LetsGetBent 

Hey Sudsy, one more question about the reply you gave me regarding the 350 Penn. You had mentioned "mag the reel" in your response. Could you please expand on this. I understand the concept but I'm not sure I can figure out where to place the magnets or how they would or could be adjusted. Thanks

Since the 350 is a reel you'll be using for weight n bait rather then plugging you can go the easy route and use a single larger magnet rather then using an adjustable style with 3 or 4 removable mags.

Here's how I did mine:




First, take a sledgehammer to an old dead hard drive and remove the rare earth magnets inside. (I really enjoyed this part. When that HD died it screwed me over badly) One of the magnets is shown in the bottom of the picture

Epoxy the magnet in place as shown on the picture.

Re assemble the reel and give the spool a spin. Chances are that it'll rub.
I VERY CAREFULLY sand it down on a benchtop belt sander untill it just clears the spool

3 coats of sally hanson nail polish to keep it from rusting and your done. 

__________________
"I just wanta play everyday despite small nagging injuries --
and go home to a woman who appreciates how full of crap I truly am"..... Crash Davis 




	  #5   

[image: image79.png]


08-23-2007, 02:45 PM 

	

Striperjim [image: image81.png]



Registered User

[image: image82.png]



 

Join Date: Mar 2004

Location: Planet Earth

Posts: 4,455 



	[image: image83.png]


Re: The Penn Reel Project - Help Fill in the Blanks 



Article on 
Do it yourself squidder magging 
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Re: The Penn Reel Project - Help Fill in the Blanks 



SCHEMATICS AND PARTS LIST POST 
Some of the more commonly used Penn reels. 

Printables. 


Discontinued reels

· Penn 704Z-705Z
· Penn 710Z - 711Z
· Penn 4500SS-5500SS
· Penn 6500SS
· Penn 7500SS-8500SS
· Penn 9500SS
· Penn 420SS-430SS
· Penn 450SS
· Penn 550SS LD
· Penn 650SS
· Penn 750SS-850SS
Popular surf and inshore Conventional / Multipliers

· Penn 525 Mag
· Squidder 140L
· 85 SeaBoy
· SeaBoy 185
· Penn 320 LD
· Penn 321 GTI
· Penn Senator 113
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Re: The Penn Conventional Reel Project - Help Fill in the Blanks 



Hi Folks,

I'm new to the board here, but specs on just about every reel that Penn made can be found at:

http://store.scottsbt.com/Penn-Reel-...ons-W32C1.aspx

Looking forward to reading the posts,

Rainier 
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Re: The Penn Conventional Reel Project - Help Fill in the Blanks 
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Re: The Penn Conventional Reel Project - Help Fill in the Blanks 



How does coat of sally hanson nail polish keep the reel save from rusting and dust. I am not cleared yet. 

__________________
home and office furniture and discounted ladies watches and shoes 
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Re: The Penn Conventional Reel Project - Help Fill in the Blanks 



Does anyone know if the Newell 338 base will fit on a 140 Squidder? If I use an Accu frame for the 140 will I need the Accurate screws or will the stock Penn screws work? 
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Re: The Penn Conventional Reel Project - Help Fill in the Blanks 



If someone with buttons could put this with the Penn 99 Silver beach please



__________________
"I just wanta play everyday despite small nagging injuries --
and go home to a woman who appreciates how full of crap I truly am"..... Crash Davis 
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Re: The Penn Conventional Reel Project - Help Fill in the Blanks 



The red spool on the 500S Penn jigmaster was an additional item that you could buy as an addon. I just recently found my old left handed Jigmaster that I bought when I was about 17, and it had the red spool on it. I found the original spool in the box that the red spool came in, and I seem to remember buying the extra spool because I wanted to have a second one with lighter line on it. The red one still has heavy line on it, and the original one has lighter stuff, both about 45 years old! Probably should buy new line... 
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Re: The Penn Conventional Reel Project - Help Fill in the Blanks 



You listed the Penn Levelmatic 920, 930, & 940 . . . There is also a 910 model . 





